E-MAIL TRANSMISSION
EUROVAC
  116 Buttermill Ave.
Concord, Ontario L4K 3X7
Tel: 905-738-9255
E-mail: bretter@eurovac.com

Date: Aug. 13, 2008	From: Burt Retter	
To: Ken Haga	Company: IAQ	
E-mail #: khaga@iaqsales.com	Pages: 	

Thank you for giving us an opportunity to quote on a Eurovac dust extraction system that will handle 9 technicians vacuuming with a 2" vacuum hose.

CFM Assumption: (based on a velocity of 5500 ft per minute)

9 technicians vacuuming w/2" vacuum hoses @ 120 CFM ea = 1080 CFM

Vacuum Assumption:

6" of HG to offset pressure losses for a longest run of 175 ft.

From the information provided to us, we recommend the following equipment:

* 40-304222, 3 phase 220 or 480 volt, centrifugal exhauster with 30 H.P. T.E.F.C. motor  capable of producing 1100 S.C.F.M. at 6.0" HG (see attached specs on motor/blower units).

*discharge silencer

* 30" x 84" primary cyclonic separator with three secondary 9" x 36" cartridge filters (210 sq ft filter area - 99.93% efficient to 3 microns) with automatic on-line and off-line compressed air pulse jet cleaning and 30 gallon collection canister (see enclosed drawings and specs).

* Vacuum relief valve 

* Electrical control panel for the 30 H.P. motor and the automatic compressed air pulse jet cleaning. Includes magnetic starter, overload protection with panel mounted stop/start and remote stop/start capability.

* 6" 16 gauge graduated galvanized tubing tubing and fittings between the pump and separator

Your cost for the above is $14,130.

Terms: 1/3 with the order,  balance on completion of installation.

Freight: FOB our Concord (suburb of Toronto), Ontario Canada plant

Please call me at 800-265-3878 ext 224 if you have any questions. 

br-iaqkenhaga.wpd